IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2020-10-02T14:16:39"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.4.0.0 - Alternate UI 18.4.0.0"
Application: "Autodesk Revit 2018 (ENG)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENG)"

People and organizations
  Person "elisabeth.kitumaini" of Organization (no name given)
  Owner history of Person "elisabeth.kitumaini" of Organization (no name given) | application "Autodesk Revit 2018 (ENG)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENG)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "AN51AluminiumStairNosings3200mm" | object type "NBS_CAT-CarpetAccessoryTrims-Limited_RgdStrNsngs_AN51AluminiumStairNosings:AN51AluminiumStairNosings3200mm" | names: "NBS_CAT-CarpetAccessoryTrims-Limited_RgdStrNsngs_AN51AluminiumStairNosings:AN51AluminiumStairNosings3200mm:22381" | material: materials ("NBS_CAT-CarpetAccessoryTrims-Limited_Aluminum_Silver", "NBS_CAT-CarpetAccessoryTrims-Limited_Aluminum_Anodized_Black") | property sets: BOS_General, NBS_Data, Pset_CoveringFlooring, Pset_CoveringCommon, IFC, COBie

Types
  IFCBUILDINGELEMENTPROXYTYPE "AN51AluminiumStairNosings3200mm" | USERDEFINED | 1 occurrence | material: materials ("NBS_CAT-CarpetAccessoryTrims-Limited_Aluminum_Silver", "NBS_CAT-CarpetAccessoryTrims-Limited_Aluminum_Anodized_Black") | property sets: BOS_General, NBS_Data, Pset_CoveringFlooring, Pset_CoveringCommon, IFC, COBie

Property sets
  BOS_General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CAT-CarpetAccessoryTrims-Limited_RigidStairNosings_AN51AluminiumStairNosings3200mm" (IFCTEXT)
    ManufacturerName = "CAT (Carpet Accessory Trims) Limited" (IFCTEXT)
    ManufacturerURL = "www.thecatweb.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/gqm2n01k" (IFCTEXT)
    NBSDescription = "Rigid stair nosings" (IFCTEXT)
    NBSReference = "45-20-35/390" (IFCTEXT)
    ProductInformation = "https://www.thecatweb.com/technical-data" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_35_90_31_74" (IFCTEXT)
    Uniclass2015Title = "Rigid stair nosings" (IFCTEXT)
    Uniclass2015Version = "Products v1.17" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Accessories = "n/a" (IFCTEXT)
    Applications = "For abutting to carpet and carpet tiles to finish the nose edge of stairs. Can be rebated to sit flush in wooden steps" (IFCTEXT)
    BaseSectionFinishOptions = "Mill, Polished, Satin" (IFCTEXT)
    BaseSectionMaterial = "Aluminium alloy 6063 T6" (IFCTEXT)
    FixingOptions = "Can be supplied pre-drilled and countersunk in the channel for concealed fixing and on-site retro fitting of the infill. Can also be supplied undrilled for adhesive fixing using F. Ball & Co. Ltd Stycco Flex Rapid Curing Flexible Adhesive" (IFCTEXT)
    InsertsColourOptions = "Dependent on infill, consult manufacturer's literature" (IFCTEXT)
    InsertsMaterialOptions = "ATI49.5, Castellated PVC, Olympic grip carborundum, Smooth textured PVC" (IFCTEXT)
    Profile = "Single channel/ square front" (IFCTEXT)
    SizeGauge = "5 mm" (IFCTEXT)
    SizeRiseXGoing = "32 x 62 mm" (IFCTEXT)
  Pset_CoveringFlooring | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    HasAntiStaticSurface = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = TRUE (IFCBOOLEAN)
  Pset_CoveringCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  IFC | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IfcExportAs = "IfcBuildingElementProxyType" (IFCTEXT)
    IfcExportType = "USERDEFINED" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_35_90_31_74:Rigid stair nosings" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Aluminium stair nosing with slip resistant infill" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "sales@cat-accs.com" (IFCTEXT)
    Material = "Aluminium alloy 6063 T6" (IFCTEXT)
    ModelNumber = "AN51" (IFCTEXT)
    ModelReference = "AN51 aluminium stair nosings 3200 mm" (IFCTEXT)
    Name = "RigidStairNosings_AN51AluminiumStairNosings3200mm_CATLimited" (IFCTEXT)
    NominalHeight = 32.00000004864 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 3200.000004864 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 62.00000009424 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "32 x 62 x 3200 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_35_90_31_74:Rigid stair nosings" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Aluminium stair nosing with slip resistant infill" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "sales@cat-accs.com" (IFCTEXT)
    Material = "Aluminium alloy 6063 T6" (IFCTEXT)
    ModelNumber = "AN51" (IFCTEXT)
    ModelReference = "AN51 aluminium stair nosings 3200 mm" (IFCTEXT)
    Name = "RigidStairNosings_AN51AluminiumStairNosings3200mm_CATLimited" (IFCTEXT)
    NominalHeight = 32.00000004864 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 3200.000004864 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 62.00000009424 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "32 x 62 x 3200 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)

Other addresses and roles
  2 x postal address (none given)